General Construction Site Hazard Detection Code Workflow

1. Run Yolo V7 on Frames to identify workers and output bounding box dimensions and positions
2. Run updatedpixel2world, reading in bounding box information and picking hazard and worksite boundary points. Outputs individual construction site map frames stored in project images directory.
3. Load project images into VideoGenerator.py to stich the images into output video.
   1. Output Video stored as MAPS.mp4